{Audi A3 (8P)} 
The Audi A3 (8P) uses 2 different communication possibilities for self diagnostics, on the one hand diagnstics via K-Line, but only for engine electronics and autom. trasmission.
Self diagnostics should be done with a CAN capable diagnostic tool.
The following control modules are build into the A3 (8P) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):

- Airbag
- Auxiliary Heater
- Brake Electronics
- CAN-Gateway
- Central Electronics
- Comfort System
- Door Control Modules
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
- Parking Aid
- Radio-/Navigation System (RNS-E)
- Steering Wheel Electronics
- Trailer
- Transmission Electronics

{CAN-Gateway}

Control Module Coding
Select 19 (CAN-Gateway)
Long Coding -> Function 07
	Byte 00 Bit 0
	Engine (Address 01)

	Byte 00 Bit 1
	Auto. Transmission (Address 02)

	Byte 00 Bit 2
	Brake Electronics (Address 03)

	Byte 00 Bit 3
	Steering Angle Sensor (G85) 

	Byte 00 Bit 4
	Airbag (Address 15)

	Byte 00 Bit 5
	Steering Aid (Address 44)

	Byte 00 Bit 6
	Xenon Range (Address 55)

	Byte 00 Bit 7
	All Wheel Drive (Address 22)

	Byte 01 Bit 0
	Central Electronics (Address 09)

	Byte 01 Bit 1
	Central Convenience (Address 46)

	Byte 01 Bit 2
	Door Electronics (Driver - Address 42)

	Byte 01 Bit 3
	Door Electronics (Passenger - Address 52)

	Byte 01 Bit 4
	Door Electronics (Rear Left - Address 62)

	Byte 01 Bit 5
	Door Electronics (Rear Right - Address 72)

	Byte 01 Bit 6
	Seat Memory Driver (Address 36)

	Byte 01 Bit 7
	Tire Pressure Monitoring (Address 65)

	Byte 02 Bit 0
	Steering Wheel Electronics (Address 16)

	Byte 02 Bit 1
	Auto HVAC (Address 08)

	Byte 02 Bit 2
	Parking Assistant (Address 76)

	Byte 02 Bit 3
	Auxiliary Heating (Address 7D)

	Byte 02 Bit 4
	Auxiliary Heating (Address 18)

	Byte 02 Bit 5
	Auto Roof (Address 26)

	Byte 02 Bit 6
	Trailer (Address 69)

	Byte 02 Bit 7
	Seat Memory Passenger (Address 06)

	Byte 03 Bit 0
	Special Function (Address 3D)

	Byte 03 Bit 1
	Sound System (Address 47)

	Byte 03 Bit 2
	Telematics (Address 75)

	Byte 03 Bit 3
	Navigation (Address 37)

	Byte 03 Bit 4
	TV-Tuner (Address 57)

	Byte 03 Bit 5
	Digital Radio (Address 0F)

	Byte 03 Bit 6
	Radio (Adress 56)

	Byte 03 Bit 7
	Telephone (Address 77)

	Byte 04 Bit 0 
	Instrument Cluster (Address 17)

	Byte 04 Bit 1
	Immobilizer (Address 25)

	Byte 04 Bit 2 
	CAN-Gateway (Address 19)
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{Central Electronics}

Control Module Coding
Select 09 (Central Electronics)
Coding -> Function 07
NOTE: This control module uses a long coding. Bytes 4 and 17-20 are only avialiable for cars from calendar week 45/2004.

	Byte 00 Bit 0
	Fog Lights installed (PR-8WB)

	Byte 00 Bit 1
	Xenon Headlights installed 

	Byte 00 Bit 2
	Footwell Lights installed (PR-QQ4)

	Byte 00 Bit 3
	Daytime Running Lights (Scandinavia)

	Byte 00 Bit 4
	Daytime Running Lights (North America)

	Byte 00 Bit 5
	Assistance Driving Light & Leaving Home

	Byte 00 Bit 6
	Rain/Light Sensor installed

	Byte 00 Bit 7
	Coming-Home

	Byte 01 Bit 0
	Rear Seat Recognition installed

	Byte 01 Bit 1
	Headlight Washer installed (PR-8X1)

	Byte 01 Bit 2
	Electronic Fuelpump Relay installed (Gasonline only)

	Byte 01 Bit 3
	Rear Wiper installed

	Byte 01 Bit 4
	Heated Side Mirror installed

	Byte 01 Bit 5
	Rear Lid Remote Opening

	Byte 01 Bit 6
	Rear Lid Remote Opening - Release

	Byte 01 Bit 7
	Rear Wiper with Front Wiper continiously active 

	Byte 02 Bit 0
	Rear Wiper with Front Wiper intermittent active

	Byte 02 Bit 1
	Comfort Turn Signals

	Byte 02 Bit 2
	Cold Lamp Diagnosis active

	Byte 02 Bit 3
	Load Management active

	Byte 02 Bit 4
	Coming-Home via
(1 = Potentiometer / 0 = Adaptation)

	Byte 02 Bit 5
	Rear Lid Remote Openening
(1 = Contact activated / 0 = Impuls activated)

	Byte 02 Bit 6
	Side Turn Signal Lights installed

	Byte 02 Bit 7
	Seat Heating installed (PR-4A3/4A4)

	Byte 03 Bit 0
	Realy Terminal 15 installed (with 2nd Battery)

	Byte 03 Bit 1
	Rear Fog Lights (1 = 1 active / 0 = 2 active)

	Byte 03 Bit 2
	Reverse Driving Lights (1 = 1 active / 0 = 2 active)

	Byte 03 Bit 3
	Reverse Driving Light off when Rear Lid open

	Byte 03 Bit 4
	Xenon-Shutter installed (Bi-Xenon)

	Byte 03 Bit 5
	Teardrop Wiping active

	Byte 03 Bit 6
	2nd Battery installed

	Byte 03 Bit 7
	Rear Lights (1 = Back Light/Brake Light dimmed / 0 = Back Light dimmed)

	Byte 04 Bit 0
	Auxiliary Heating installed

	Byte 04 Bit 1
	Auxiliary Heating installed

	Byte 04 Bit 2
	Trailer/Towing Device installed

	Byte 04 Bit 3
	Memory Seats installed

	Byte 04 Bit 4
	Activation of both Rear Fog Lights

	Byte 04 Bit 5
	Model (0 = Right Hand Drive / 1 = Left Hand Drive)

	Byte 04 Bit 6
	Rear Fog Lights deactivated

	Byte 04 Bit 7
	Climatronic installed

	Byte 05
	Headlight Washer Delay
(Standard: 1000 ms / Resolution: 50 ms)

	Byte 06
	Headlight Washer Activation Time
(Standard: 800 ms / Resolution: 50 ms)

	Byte 07
	Extra Function: Turn Signal Front left/right as Parking Light Front left/right (USA and Canada)

	Byte 08
	Extra Function: Low Beam left/right as Daytime Running Light - Scandinavia (Standard: 0%)

	Byte 09
	Extra Function: Brake Light left/right Rear as Parking Light (Standard: 18%)

	Byte 10
	Extra Function: Rear Fog Light left/right as Parking Light (Standard: 12%)

	Byte 11
	Extra Function: Front Parking Light left/right (Standard: 0%)

	Byte 12
	Extra Function: Rear Parking Light left/right (Standard: 0%)

	Byte 13
	Replacement Function: Front Side Turn Signal left/right as Front Parking Light (Standard: 0%)

	Byte 14
	Replacement Function: Front Parking Light left/right as Side Turn Signals left/right (Standard: 0%)

	Byte 15
	Replacement Function: Rear Light left/right as Side Turn Signals left/right (Standard: 0%)

	Byte 16
	Replacement Function: Front Fog Lights left/right as Low Beam Headlight left/right (Standard: 0%)

	Byte 17 Bit 0
	Ermergency Brake Flash Light active

	Byte 17 Bit 1
	Deactivation of Additional High Beam with Bi-Xenon

	Byte 17 Bit 2
	Heated Front Window installed

	Byte 17 Bit 3
	Diagnostics Terminal 50 active

	Byte 17 Bit 4
	Daylight Running Light with dimmed Low Beam

	Byte 17 Bit 5
	Front Fog Lights deactivated with High Beam

	Byte 17 Bit 6
	Parking Light Function inactive (USA/Canada)

	Byte 17 Bit 7
	reserved

	Byte 18 Bit 0
	Cold Diagnosis License Plate Lights active

	Byte 18 Bit 1
	Cold Diagnosis Brake Lights active

	Byte 18 Bit 2
	Cold Diagnosis Front Fog Lights active

	Byte 18 Bit 3
	Cold Diagnosis Rear Fog Lights active

	Byte 18 Bit 4
	Cold Diagnosis High Beam active

	Byte 18 Bit 5
	Cold Diagnosis Turn Signals active

	Byte 18 Bit 6
	Cold Diagnosis Back Light active

	Byte 18 Bit 7
	Cold Diagnosis Side Turn Signals active

	Byte 19 Bit 0
	Cold Diagnosis Low Beam active

	Byte 19 Bit 1
	Cold Diagnosis Front Parking Lights active

	Byte 19 Bit 2
	Cold Diagnosis Rear Parking Lights active

	Byte 19 Bit 3
	Diagnosis Rear Parking Lights active

	Byte 19 Bit 4
	unknown/unused

	Byte 19 Bit 5
	unknown/unused

	Byte 19 Bit 6
	unknown/unused

	Byte 19 Bit 7
	unknown/unused

	Byte 20
	unknown/unused
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{Comfort System}

Control Module Coding
Select 46 (Comfort System)
Long Coding -> Function 07
	Byte 00 Bit 0
	Selective Central Locking 

	Byte 00 Bit 1
	Central Locking w/o Safe-Function 

	Byte 00 Bit 2
	Central Locking w/o sensible 

	Byte 00 Bit 3
	Auto-Unlock (unlocking after removing key from ignition)

	Byte 00 Bit 4
	Auto-Lock (autom. locking above 10 mph)

	Byte 00 Bit 5
	not relevant/unused

	Byte 00 Bit 6
	not relevant/unused

	Byte 00 Bit 7
	not relevant/unused

	Byte 01 Bit 0
	not relevant/unused

	Byte 01 Bit 1
	not relevant/unused

	Byte 01 Bit 2
	not relevant/unused

	Byte 01 Bit 3
	not relevant/unused

	Byte 01 Bit 4
	not relevant/unused

	Byte 01 Bit 5
	not relevant/unused

	Byte 01 Bit 6
	not relevant/unused

	Byte 01 Bit 7
	not relevant/unused

	Byte 02 Bit 0
	not relevant/unused

	Byte 02 Bit 1
	not relevant/unused

	Byte 02 Bit 2
	not relevant/unused

	Byte 02 Bit 3
	not relevant/unused

	Byte 02 Bit 4
	not relevant/unused

	Byte 02 Bit 5
	not relevant/unused

	Byte 02 Bit 6
	not relevant/unused

	Byte 02 Bit 7
	not relevant/unused

	Byte 03 Bit 0
	Comfort function inactive

	Byte 03 Bit 1
	Comfort function power windows/sunroof via door lock drivers door inactive

	Byte 03 Bit 2
	Comfort function power windows/sunroof via door lock passengers door inactive

	Byte 03 Bit 3
	Comfort function power windows/sunroof via door lock rear lid inactive

	Byte 03 Bit 4
	Comfort function power windows/sunroof via power window switch in drivers door inactive

	Byte 03 Bit 5
	Comfort function power windows/sunroof via remote control inactive

	Byte 03 Bit 6
	Comfort function autom. closing 

	Byte 03 Bit 7
	Power windows/sunroof disabled after door opening

	Byte 04 Bit 0 
	Comfort opening power windows via door lock active

	Byte 04 Bit 1
	Comfort opening power windows via power window switch active

	Byte 04 Bit 2
	Comfort opening power windows via remote control active

	Byte 04 Bit 3
	Comfort closing power windows via door lock active

	Byte 04 Bit 4
	Comfort closing power windows via power window switch active

	Byte 04 Bit 5
	Comfort closing power windows via remote control active

	Byte 04 Bit 6
	Comfort function after authorized access only in a limited time 

	Byte 04 Bit 7
	not relevant/unused

	Byte 05 Bit 0
	Comfort opening sunroof via door lock active

	Byte 05 Bit 1
	Comfort opening sunroof via power window switch active

	Byte 05 Bit 2
	Comfort opening sunroof via remote control active

	Byte 05 Bit 3
	Comfort closing sunroof via door lock active

	Byte 05 Bit 4
	Comfort closing sunroof via power window switch active

	Byte 05 Bit 5
	Comfort closing sunroof via remote control active

	Byte 05 Bit 6
	not relevant/unused

	Byte 05 Bit 7
	not relevant/unused

	Byte 06 Bit 0
	Unlocking Confirmation (Blink) via Door Locks

	Byte 06 Bit 1
	Unlocking Confirmation (Horn) via Door Locks

	Byte 06 Bit 2
	Unlocking Confirmation (Blink) via Remote Control

	Byte 06 Bit 3
	Unlocking Confirmation (Horn) via Remote Control

	Byte 06 Bit 4
	not relevant/unused

	Byte 06 Bit 5
	not relevant/unused

	Byte 06 Bit 6
	not relevant/unused

	Byte 06 Bit 7
	Adaptation of Horn Confirmation locked

	Byte 07 Bit 0
	Locking Confirmation (Blink) via Door Locks

	Byte 07 Bit 1
	Locking Confirmation (Horn) via Door Locks

	Byte 07 Bit 2
	Locking Confirmation (Blink) via Remote Control

	Byte 07 Bit 3
	Locking Confirmation (Horn) via Remote Control

	Byte 07 Bit 4
	not relevant/unused

	Byte 07 Bit 5
	not relevant/unused

	Byte 07 Bit 6
	not relevant/unused

	Byte 07 Bit 7
	not relevant/unused

	Byte 08 Bit 0
	Remote control inactive

	Byte 08 Bit 1
	Remote control with "Terminal 15 ON" inactive

	Byte 08 Bit 2
	Remote control range limitation active

	Byte 08 Bit 3
	Manual remote control lerning/unlearning active

	Byte 08 Bit 4
	not relevant/unused

	Byte 08 Bit 5
	not relevant/unused

	Byte 08 Bit 6
	Activation Blink Signal (Anti-Theft-Warning System) 

	Byte 08 Bit 7
	Activation Horn Signal (Anti-Theft-Warning System)

	Byte 09 Bit 0
	Doors (0 = 2-doors / 1 = 4-doors)

	Byte 09 Bit 1
	Power windows front installed

	Byte 09 Bit 2
	Power windows rear installed

	Byte 09 Bit 3
	Central locking installed 

	Byte 09 Bit 4
	Model (0 = Left Hand Drive/ 1 = Right Hand Drive)

	Byte 09 Bit 5
	not relevant/unused

	Byte 09 Bit 6
	Synchronous mirror adjustment

	Byte 09 Bit 7
	Mirror lowering with reverse gear
(only with Memory Seats)

	Byte 10 Bit 0
	Anti-theft system deactivated

	Byte 10 Bit 1
	Anti-theft system disarming only via remote control or immobilizer

	Byte 10 Bit 2
	not relevant/unused

	Byte 10 Bit 3
	Anti-theft alarm delay (15 s) inactive (Thatcham)

	Byte 10 Bit 4
	not relevant/unused

	Byte 10 Bit 5
	Anti-theft system passive arming

	Byte 10 Bit 6
	Inclination Sensor installed

	Byte 10 Bit 7
	Interior Monitoring installed

	Byte 11 Bit 0
	not relevant/unused

	Byte 11 Bit 1
	not relevant/unused

	Byte 11 Bit 2
	not relevant/unused

	Byte 11 Bit 3
	not relevant/unused

	Byte 11 Bit 4
	Siren installed

	Byte 11 Bit 5
	Siren Tone Type
(0 = frequency modulated / 1 = intermittent)

	Byte 11 Bit 6
	Siren Alarm Type
(0 = 10 "tamper" alarms / 1 = 1 "tamper" alarm)

	Byte 11 Bit 7
	not relevant/unused

	Byte 12 Bit 0
	Rear door warning lights installed

	Byte 12 Bit 1
	not relevant/unused

	Byte 12 Bit 2
	not relevant/unused

	Byte 12 Bit 3
	not relevant/unused

	Byte 12 Bit 4
	not relevant/unused

	Byte 12 Bit 5
	not relevant/unused

	Byte 12 Bit 6
	not relevant/unused

	Byte 12 Bit 7
	not relevant/unused


 

Control Module Adaptation
Select 46 (Comfort System)
Adaptation -> Function 10
-> Channel 000 (Remote Control - Erasing)
Erase all keys.

-> Channel 001 (Remote Control - Key Matching)
Adaptation of remote controls, 1-4 Keys.

-> Channel 003 (Selective Locking)
0 - Unlocking of all Doors
1 - Selective Unlocking

-> Channel 004 (Auto-Lock)
The doors will lock automatically when the vehicle reaches a speed of 15 km/h or 10 mph (0 = off/1 = on).

-> Channel 005 (Auto-Unlock)
The doors will unlock automatically when the key is removed from the ignition switch (0 = off/1 = on).

-> Channel 007 (Unlock Message - Remote)
Return message when unlocking via remote control.

0 - No return message
1 - Beep
2 - Blink
3 - Beep & Blink

-> Channel 008 (Unlock Message - Key)
Return message when unlocking via key switch.

0 - No return message
1 - Beep
2 - Blink
3 - Beep & Blink

-> Channel 010 (Lock Message - Remote)
Return message when locking via remote control.

0 - No return message
1 - Beep
2 - Blink
3 - Beep & Blink

-> Channel 011 (Lock Message - Key)
Return message when locking via key switch.

0 - No return message
1 - Beep
2 - Blink
3 - Beep & Blink

-> Channel 012 (Activation Message - Anti-Theft)
Return message when anti theft warning system is active.

0 - No return message
1 - Beep
2 - Blink
3 - Beep & Blink

-> Channel 013 (Alarm Horn)
Country setting for alarm horn.

	0
	Siren Tone Type: frequency modulated
Siren Alarm Type: 10 "tamper" alarms

	1
	Siren Tone Type: frequency modulated
Siren Alarm Type: 1 "tamper" alarm

	2
	Siren Tone Type: intermittend
Siren Alarm Type: 10 "tamper" alarms

	3
	Siren Tone Type: intermittend
Siren Alarm Type: 1 "tamper" alarm


-> Channel 014 (Inclination Sensor Sensitivity)
100 = 50 %
140 = 70 %
200 = 100 %

-> Channel 015 (Interior Monitoring Sensitivity)
100 = 50 %
140 = 70 %
200 = 100 %

-> Channel 016 (Battery Monitoring - Sounder)
0 = off
5 = on

-> Channel 017 (Comfort Function)
This function activates/deactivates the comfort function via remote (0 = off/1 = on). See long coding for more details/options.

-> Channel 018 (Anti-Theft Delay)
Deactivation of the anti theft warning delay, when opening drivers door, before the anti theft warning system is beeing activated (1 = off/0 = on).
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{Steering Wheel Electronics}

Control Module Coding
Select 16 (Steering Wheel Electronics)
Coding -> Function 07
00?xxxx: Transmission
0 - Manual Transmission
1 - Automatic Transmission

00x?xxx: Steering Wheel
0 - 3-Spoke, w/o Tiptronic, w/o Multi-Function
1 - 3-Spoke, with Tiptronic, w/o Multi-Function
2 - 4-Spoke Multi-Function (with Radio Control)
3 - 4-Spoke Multi-Function (with Radio/Telephone Control)
4 - 4-Spoke Multi-Function (with Radio/Telephone/Voice Control)
00xx?xx: Tiptronic/Heating
+1 - Tiptronic on Steering Wheel
+2 - Steering Wheel Heating

00xxx?x: Cruise Control/Board Computer
0 - no Board Computer, no Cruise Control
1 - Board Computer, no Cruise Control
2 - no Board Computer, Cruise Control
4 - Board Computer, Cruise Control

00xxxx?: Rear Wiper
0 - w/o Rear Wiper
1 - with Rear Wiper

{Audi A4 (8D)} 
The following control modules are build into the A8 (4D) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):
- Airbag
- Autom. Transmission
- Auxiliary Heater
- Brake Electronics
- Central Locking/Comfort System
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
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{Engine Electronics}

Control Module Coding (AEB)
Select 01 (Engine Electronics)
Coding -> Function 07
??xxx: Country/Emissions
02 - non-EU (MVEG I)
04 - EU (MVEG II)
06 - USA (with EVAP system leak detection pump)
08 - China and CIS (Commonwealth of Independent States)
25 - Japan (< 06/96)
xx?xx: Drivetrain/Options
0 - Front-wheel-drive w/o traction control (ASR)
1 - Front-wheel-drive with traction control (ASR)
2 - All-wheel-drive w/o traction control (ASR)
3 - All-wheel-drive with traction control (ASR)
xxx?x: Transmission
0 - 5-speed manual transmission
3 - Automatic transmission
5 - Automatic transmission (01V)
xxxx?: Vehicle type
1 - Audi A4
2 - Audi A6
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{Instrument Cluster}

Control Module Coding
Select 17 (Instrument Cluster)
Coding -> Function 07
??xxx: Extra-Options (through MY 1999)
+00 - no Extra Options 
+01 - Brake pad warning active
+02 - Seatbelt warning active
+04 - Washer fluid warning active
+16 - Navigation active
??xxx: Extra-Options (from MY 2000)
+00 - no Extra Options or Nav. III
+02 - Seatbelt warning active
+16 - Navigation I & II 
xx?xx: Country
0 - Germany (D)
1 - Europe (EU) (through MY 1999)
1 - Rest of World (left hand steering - RoW) (from MY 2000)
2 - USA (US)
3 - Canada (CDN)
4 - Great Britain (GB)
5 - Japan (JP) (through MY 1999)
5 - Japan (left hand steering - JP) (from MY 2000)
6 - Saudi Arabia (SA)
7 - Australia (AUS)
8 - Rest of World (right hand steering - RoW) (from MY 2000)
9 - Japan (right hand steering - JP) (from MY 2000)
xxx?x: Cylinder 
4 - 4-Cylinder
6 - 6-Cylinder
8 - 8-Cylinder 
xxxx?: Engine
0 - TDI-Engine
2 - 4-Cylinder and 6-Cylinder Gasoline-Engine 
3 - 8-Cylinder Gasoline-Engine
4 - Turbo-Engine (from MY 2000)
	
	{Audi A4 (8E)} 
The following control modules are build into the A4 (8E) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):
- Airbag
- Autom. Transmission
- Auxiliary Heater
- Brake Electronics
- Central Electronics
- Comfort System
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
- Parking Aid
- Radio-/Navigation System (RNS-E)
- Steering Wheel Electronics
- Tire Pressue Monitoring
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{Autom. Transmission}

Control Module Coding
Select 09 (Autom. Transmission)
Coding -> Function 07
000?0xx: Tiptronic/Paddels
0 - not installed
1 - installed

000x0?x: Dynamic Shift Program (DSP)
0 - active
1 - inactive

000x0x?: Country/Drivetrain
1 - Rest of World (RoW) / All-Wheel-Drive (AWD)
2 - North America (NAR) / All-Wheel-Drive (AWD)
3 - Rest of World (RoW) / Front-Wheel-Drive (FWD)
4 - North America (NAR) / Front-Wheel-Drive (FWD)
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{Brake Electronics}

Control Module Coding II/Login (Bosch 5.7)
Note #1: After Login/Coding-II has been carried out, you need to recode the control module.
Note #2: Special Login/Coding-II 09399 is used for BFB Engine with 1LT Brakes and Multitronic.

Select 03 (Brake Electronics)
Coding II/Login -> Function 11
0?xxx: Chassis
9 - Audi A4

0x?xx: Brakes
2 - Brembo 17" (PR-1LJ)
3 - FN3 16" (PR-1LT/1LF)
4 - HP2 16" (PR-1LX)
4 - FNR 16" (PR-1LA/1LG)
5 - FN3 15" (PR-1LB/1LE)
6 - C54 (PR-1LZ)
0xx?x: Engine
5 - 4/6 Cyl. Diesel
7 - 4/5 Cyl. Gasoline 
9 - 6/8 Cyl. Gasoline

0xxx?: Transmission
5 - Manual
7 - Automatic (5HP19, 5HP24, AG4, AG5)
9 - Multitronic

 

Control Module Coding (Bosch 5.7)
Note #1: Coding is accepted after a specific login has been carried out.
Note #2: After succesful coding the steering angle sensor basic setting needs to be carried out.
Note #3: Special Coding 04499 is used for BFB Engine with 1LT Brakes and Multitronic.

Select 03 (Brake Electronics)
Coding -> Function 07
0?xxx: Chassis
4 - Audi A4

0x?xx: Brakes
1 - C54 (PR-1LZ)
2 - FN3 15" (PR-1LB/1LE)
3 - HP2 16" (PR-1LX)
3 - FNR 16" (PR-1LG)
4 - FN3 16" (PR-1LT/1LF)
5 - Brembo 17" (PR-1LJ)
0xx?x: Engine
5 - 4/6 Cyl. Diesel
7 - 4/5 Cyl. Gasoline
9 - 6/8 Cyl. Gasoline

0xxx?: Transmission
5 - Manual
7 - Automatic (5HP19, 5HP24, AG4, AG5)
9 - Multitronic

 

Control Module Coding (Bosch 8.0)
Note #1: There is no Login/Coding-II necessary.
Note #2: After succesful coding the steering angle sensor basic setting needs to be carried out.

Select 03 (Brake Electronics)
Coding -> Function 07
On Request.
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{Central Electronics}

Control Module Coding (only 8EC/8ED)
Select 09 (Central Electronics)
Coding -> Function 07
?xxxx: Chassis
0 - Limousine
1 - Avant

x?xxx: Driving Light Switch
0 - without Rain/Light Sensor (G397)
1 - with Rain/Light Sensor (G397)
xx?xx: Trailer Hitch
0 - without Trailer Hitch
1 - with Trailer Hitch

xxx?x: Headlights
0 - Halogen Headlights w/o Daytime Running Lights
1 - Halogen Headlights with Daytime Running Lights
2 - Bi-Xenon Headlights with Daytime Running Lights
3 - Bi-Xenon Headlights w/o Daytime Running Lights
4 - Bi-Xenon Headlights with Daytime Running/Tail/License Plate Lights

xxxx?: Country
1 - Rest of World/Nordic Countries/Denmark/Croatia/Baltic Countries with Bi-Xenon
2 - Nordic Countries/Denmark/Croatia/Baltic Countries without Bi-Xenon
3 - USA/Canada with Bi-Xenon
4 - Canada without Bi-Xenon
5 - Special Vehicles
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{Comfort System}

Control Module Coding
Select 46 (Comfort System)
Coding -> Function 07
+00001 - 10 Tamper alarms (Great Britain)
+00002 - Confirmation Anti-theft warning system blinks
+00004 - Selective Central Locking (SCL)
+00008 - Anti-theft warning system - activation of AWS
+00016 - Rear lid release locking via speed
+00032 - Comfort Locking via speed
+00064 - Comfort function via remote control
+00128 - Right Hand Drive (RHD)
+00256 - Avant bit
+00512 - Confirmation remote closing (1x blink)
+01024 - Confirmation anti-theft warning sytem horn activation
+02048 - Door-/ window regulator logic
+04096 - Thatcham anti-theft warning
+08192 - No safe-function 
+16384 - Side windows with insulated glass

 

Control Module Adaptation 
Select 46 (Comfort System)
Adaptation -> Function 10
-> Channel 61 (Variants Reduction)
0 - w/o light package / four door control modules (PR-QQ0/4R4)
1 - w/o light package / mech. window regulators rear (PR-QQ0/4R5)
2 - with light package / four door control modules (PR-QQ1/4R4)
3 - with light package / mech. window regulators rear (PR-QQ1/4R5)
-> Channel 62 (Comfort Function)
+001 - Comfort closing via remote for window regulators (not USA)
+002 - Comfort opening via remote for window regulators (not USA)
+004 - Comfort closing via lock cylinder for window regulators
+008 - Comfort opening via lock cylinder for window regulators
+016 - Comfort closing via remote for sunroof (not USA)
+032 - Comfort opening via remote for sunroof (not realized)
+064 - Comfort closing via lock cylinder for sunroof
+128 - Comfort opening via lock cylinder for sunroof (not realized)
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{Instrument Cluster}

Control Module Coding (only 8E2/8E5)
Select 17 (Instrument Cluster)
Coding -> Function 07
??xx1: Extra-Options
+00 - 1. K-Number (Europe, USA, Rest of World)
+01 - Smaller Fuel Tank Volume (All wheel drive)
+02 - Seatbelt Warning (NAR old - NOT USA from 45/2004)
+04 - 3. K-Number (Rental Cars)
+08 - 2. K-Number (Australia)
xx?x1: Country-Setting
0 - Germany (D)
1 - Rest of World (RoW)
2 - USA (US)
3 - Canada (CAN)
4 - Great Britain (GB)
5 - Japan (JP)
6 - Saudi Arabia
7 - Australia (AUS)
xxx?1: Seatbelt Warning
0 - No Seatbelt Warning (or NAR old)
3 - Seatbelt Warning (NAR new - from Week 45/2004)
 

Control Module Coding (only 8EC/8ED)
Select 17 (Instrument Cluster)
Coding -> Function 07
??xx1: Extra-Options
+00 - 1. K-Number (Europe, USA, Rest of World)
+01 - Smaller Fuel Tank Volume (All wheel drive)
+02 - Side Marker Lights Indicator Lamp inactive
+04 - 3. K-Number (Rental Cars)
+08 - 2. K-Number (Australia)
+16 - Clutch Pedal Switch Operation in FIS Display
xx?x1: Country-Setting
0 - Germany (D)
1 - Rest of World (RoW)
2 - USA (US)
3 - Canada (CAN)
4 - Great Britain (GB)
5 - Japan (JP)
6 - Saudi Arabia
7 - Australia (AUS)
xxx?1: Seatbelt Warning
0
No Seatbelt Warning
1
Seatbelt Warning Europe-NCAP
Optical durable warning, acustical warning for 91 seconds activ.
2
Seatbelt Warning USA and Canada old 
Optical and acustical warning for 6 seconds.
3
Seatbelt Warning USA and Canada NAR neu
Optical durable warning, acustical warning all 30 seconds.
4
Seatbelt Warning Europe-NCAP (incl. passenger)
Optical durable warning, acustical warning for 91 seconds activ.
5
Seatbelt Warning USA and Canada old (incl. passenger)
Optical and acustical warning for 6 seconds.
6
Seatbelt Warning USA and Canada NAR new (incl. passenger)
Optical durable warning, acustical warning all 30 seconds.
 

Control Module Adaptation
Select 17 (Instrument Cluster)
Adaptation -> Function 10
-> Channel 19 (Misc)
xxxx?: Remote Clock
0 - Remote Clock not active
1 - Remote Clock active

xxx?x: Ambient Temperature
0 - no Display, Illumination inactive
1 - Display and Illumination active

xx?xx: Driver Information System (DIS)
0 - DIS 1
1 - Highline without DIS
2 - DIS 2

x?xxx: Board Computer
0 - only Level 2 (long time memory)
1 - Level 1 and 2

?xxxx: Illumination Option
0 - Needle and Scala only active at 'Light on"
1 - Needle already active at 'Ignition on'
2 - Scale already active at 'Ignition on'
3 - Scala (2. Map) and Needle at "ignition on" active
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{Parking Aid}

Control Module Coding (8EC/8ED)
Select 76 (Parking Aid)
Coding -> Function 07
00?xxxx: Trailer Hitch
0 - without Trailer Hitch
1 - with Trailer Hitch

00x?xxx: Transmission
0 - Manual Transmission
1 - Automatic Transmission

00xx?xx: Specification
0 - ECE Countries (without reinforced bumper)
1 - ECE-Countries (S-Model without reinforced bumper)
2 - USA (with reinforced bumper)
3 - USA (S-Model with reinforced bumper)
4 - ECE-Countries (RS-Model)
5 - USA (RS-Model)
00xxx?x: Chassis
0 - Sedan

00xxxx?: Model
4 - Audi A4 (8E)
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Last update 26.10.2005


{Audi A6 (4B)} 
The following control modules are build into the A6 (4B) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):
- Airbag
- Autom. Transmission
- Auxiliary Heater
- Brake Electronics
- Central Locking/Comfort System
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
 

{Instrument Cluster}

Control Module Coding
Select 17 (Instrument Cluster)
Coding -> Function 07
??xxx: Equipment (through MY 1999)
+01 - Brake Pad Warning active
+02 - Seatbelt Warning active
+04 - Washer Fluid Warning active
+16 - Navigation active
??xxx: Equipment (from MY 2000)
+01 - 80l Fuel Tank for 8-Cylinder and S6
+02 - Seatbelt Warning active
+04 - Tires for A6 allroad quattro
xx?xx: Country
0 - Germany (D)
1 - Europe (EU) (through MY 1999)
1 - Rest of World (left hand steering - RoW) (from MY 2000)
2 - USA (US)
3 - Canada (CDN)
4 - Great Britain (GB)
5 - Japan (JP) (through MY 1999)
5 - Japan (left hand steering - JP) (from MY 2000)
6 - Saudi Arabia (SA)
7 - Australia (AUS)
8 - Rest of World (right hand steering - RoW) (from MY 2000)
9 - Japan (right hand steering - JP) (from MY 2000)
xxx?x: Cylinder 
4 - 4-Cylinder
6 - 6-Cylinder
8 - 8-Cylinder
xxxx?: Engine
0 - TDI-Engine
2 - 4-Cylinder and 6-Cylinder Gasoline-Engine 
3 - 8-Cylinder Gasoline-Engine
4 - Turbo-Engine (from MY 2000)
 

Control Module Adaptation
Select 17 (Instrument Cluster)
Adaptation -> Function 10
-> Channel 60 (CAN-Powertrain)
+00001 - Engine (if TDI and/or MY 2001 and above)
+00002 - Automatic Transmission
+00128 - Post Shift-Step (allroad only)
+01024 - Instrument Cluster (if TDI and/or MY 2001 and above)
+02048 - Self-Levelling Suspension (allroad only)
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{Audi A6 (4F)} 
The Audi A6 (4F) uses 2 different communication possibilities for self diagnostics, on the one hand diagnstics via K-Line, but only for engine electronics and autom. trasmission.
Self diagnostics has to be done with a CAN capable diagnostic tool.
The following control modules are build into the A6 (4F) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):

- Airbag
- Access/Start Authorization
- Auxiliary Heater
- Brake Electronics
- Central Electronics
- Central Electronics 2
- Comfort System
- Control Head (front)
- Distance Regulation
- Door Control Modules
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
- Level Control System
- Parking Aid
- Parking Brake
- Roof Electronics
- Steering Wheel Electronics
- Tire Pressue Monitoring
- Trailer
- Transmission Electronics

[image: image14.jpg]



 

{Comfort System}

Control Module Coding
Select 46 (Comfort System)
Coding -> Function 07
+0000001 - Reserved (always)
+0000002 - 10 Tamper Alarms (PR-B09)
+0000004 - Thatcham inactive (PR-7AA/A8U)
+0000008 - Selective Central Locking (PR-4K2/4K7/4K8)
+0000016 - Anti-Theft Warning System (PR-7AN/7AL)
+0000032 - Inclination Sensor installed (PR-7AN/7AL)
+0000064 - Interior Monitoring (PR-7AL)
+0000128 - Comfort Function via Remote (NOT PR-B29/B30/B34/B35)
+0000256 - Right Hand Steering (PR-L0R)
+0000512 - Avant (PR-K8D)
+0001024 - Electrical Rear Shades installed (PR-3Y2/3Y5)
+0002048 - Confirmation Anti-Theft System via Horn (PR-A8U)
+0004096 - SAE Rear Lights (PR-A8U)
+0008192 - Light Package (PR-QQ1)
+0016384 - SAFE-Function deactivated (PR-A8U)
+0065536 - Anti-Theft Delay (0 Seconds)
+0131072 - Highline (LED Rear Lights)
+0262144 - Sunroof (PR-3FE/3FR)
+1048576 - Luggage Compartment Closing Assistance (PR-4E7/4E9)
+2097152 - Rear Lid Control Module (PR-4E7/4E9)
 

Control Module Adaptation
Select 46 (Comfort System)
Adaptation -> Function 10
-> Channel 001 (Personalization - Key 1)
-> Channel 002 (Personalization - Key 2)
-> Channel 003 (Personalization - Key 3)
-> Channel 004 (Personalization - Key 4)
+00001 - Passenger door
+00002 - Rear left door
+00004 - Rear right door
+00008 - Luggage compartment
+00016 - Auto-Lock/Unlock
+00032 - Comfort opening of front window regulators
+00064 - Comfort opening of rear window regulators
+00128 - Comfort opening of sunroof
+00256 - Rear shade automatic
+00512 - Interior light dimming value = 1 %
+01024 - Interior light dimming value = 2 %
+02048 - Interior light dimming value = 4 %
+04096 - Interior light dimming value = 8 %
+08192 - Interior light dimming value = 16 %
+16384 - Interior light dimming value = 32 %
+32768 - Interior light dimming value = 64 %

-> Channel 015 (Interior Monitoring Sensitivity)
200 - 100 %
180 - 90 %
160 - 80 %
140 - 70 %
120 - 60 %
100 - 50 %

-> Channel 050 (Adaptive Brake Light)
+1 - Emergency Brake Blinking
+2 - Brake Light Surface Amplification (only Sedan)
-> Channel 061 (Comfot Functions)
+001 - Comfort closing for window regulators via remote control
+002 - Comfort opening for window regulators via remote control
+004 - Comfort closing for sunroof via remote control
+008 - Comfort opening for sunroof via remote control
+016 - Comfort closing for window regulator via switch drivers door
+032 - Comfort opening for window regulator via switch drivers door
+064 - Comfort locking for sunroof via switch drivers door
+128 - Comfort opening for sunroof via switch drivers door
+256 - Comfort closing for window regulators via lock cylinder
+512 - Comfort closing for sunroof via lock cylinder

-> Channel 062 (Central Locking Functions)
+1 - Central locking closed blinking
+2 - Central locking open blinking
+4 - Terminal 87 USA logic

{Audi A8 (4D)} 
The following control modules are build into the A8 (4D) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):
- Airbag
- Autom. Transmission
- Auxiliary Heater
- Brake Electronics
- Central Locking/Comfort System
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster

[image: image15.jpg]



 

{Comfort System}

Control module coding (< 06/1997)
Select 46 (Comfort System)
Coding -> Function 07
+00004 - Selective Central Locking (SCL)
+00008 - Anti-Theft Warning System
+00032 - Comfort Locking via Speed (15 km/h / 10 mph)
+00064 - Comfort Function via Remote Control
+00128 - Dynamic Interior Monitoring
+00256 - Trunk Logic (Anti-Theft)
+00512 - Confirmation Remote Closing
+01024 - Confirmation Anti-Theft Warning Sytem (Horn)
+02048 - Door/Window Logic (USA)
+08192 - Remote Control

 

Control module coding (06/1997 > 05/2000)
Select 46 (Comfort System)
Coding -> Function 07
+00002 - Confirmation Anti-theft Warning System (Blink)
+00004 - Selective Central Locking (SCL)
+00008 - Anti-Theft Warning System
+00032 - Comfort Locking via Speed (15 km/h / 10 mph)
+00064 - Comfort Function via Remote Control
+00256 - Trunk Logic (Anti-Theft)
+00512 - Confirmation Remote Closing
+01024 - Confirmation Anti-Theft Warning Sytem (Horn)
+02048 - Door/Window Logic (USA)
+04096 - Confirmation Remote Opening
+08192 - Remote Control

 

Control module coding (05/2000 >)
Select 46 (Comfort System)
Coding -> Function 07
+00002 - Confirmation Anti-theft Warning System (Blink)
+00004 - Selective Central Locking (SCL)
+00008 - Anti-Theft Warning System
+00032 - Comfort Locking via Speed (15 km/h / 10 mph)
+00064 - Comfort Function via Remote Control
+00256 - Trunk Logic (Anti-Theft)
+00512 - Confirmation Remote Closing
+02048 - Door/Window Logic (USA)
+04096 - Confirmation Remote Opening
+08192 - Remote Control
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{Audi A8 (4E)} 
The Audi A8 (4E) uses 2 different communication possibilities for self diagnostics, on the one hand diagnstics via K-Line, but only for engine electronics and autom. trasmission.
Self diagnostics should be done with a CAN capable diagnostic tool.
The following control modules are build into the A8 (4E) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):

- Airbag
- Access/Start Authorization
- Auxiliary Heater
- Brake Electronics
- Central Electronics
- Central Electronics 2
- Comfort System
- Control Head (front)
- Distance Regulation
- Door Control Modules
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
- Level Control System
- Parking Aid
- Parking Brake
- Roof Electronics
- Steering Wheel Electronics
- Tire Pressue Monitoring
- Trailer
- Transmission Electronics
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{Comfort System}

Control module coding
Select 46 (Comfort System)
Coding -> Function 07
+00001 - 10 Tamper alarms (PR-B09)
+00002 - Thatcham anti-theft inactive
+00004 - Selective central locking (PR-4K2/4K6/4K7)
+00008 - Anti-theft warning system (PR-7AH/7AL)
+00016 - Inclination sensor installed (PR-7AL)
+00032 - Control module for rear lid installed (PR-4E7/4E9)
+00064 - Comfort function via remote
+00128 - Right hand steering (PR-L0R)
+00512 - Rear blinds installed (PR-3Y2/3Y5/3Y8)
+01024 - Confirmation anti-theft warning system via horn (PR-A8U)
+02048 - SAE rear lights (PR-A8U)
+04096 - Footwell light with LED technology (PR-QQ1/QQ3)
+08192 - SAFE-function deactivated (PR-A8U)
+16384 - Fuel filler cap recognition (PR-A8U)
+32768 - Interior monitoring (PR-A8U)
 

Control module adaptation 
Select 46 (Comfort System)
Adaptation -> Function 10
-> Channel 61 (Comfot Functions)
+001 - Comfort closing for window regulators via remote control
+002 - Comfort opening for window regulators via remote control
+004 - Comfort closing for sunroof via remote control
+008 - Comfort opening for sunroof via remote control
+016 - Comfort closing for window regulator via switch drivers door
+032 - Comfort opening for window regulator via switch drivers door
+064 - Comfort locking for sunroof via switch drivers door
+128 - Comfort opening for sunroof via switch drivers door
+256 - Comfort closing for window regulators via lock cylinder
+512 - Comfort closing for sunroof via lock cylinder

-> Channel 62 (Central Locking Functions)
+1 - Central locking closed blinking
+2 - Central locking open blinking
+4 - Terminal 87 USA logic 
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{Door Control Modules}

Control module coding
Select 42 (Door Control Module Driver)
Select 52 (Door Control Module Passenger)
Select 62 (Door Control Module Rear Left)
Select 72 (Door Control Module Rear Right)
Coding -> Function 07
+00001 - Insulated glass (PR-4KR/4KV)
+00002 - Right hand steering (PR-L0R)
+00004 - Ambient lighting (PR-QQ1/QQ3)
+00008 - Sourrinding area light (PR-QQ1/QQ3)
+00016 - Synchronous mirror adjustment
+00032 - Recirculated air-closing
+00064 - Lock with electrical child-safety lock (PR-GZ2)
+00128 - Electrical sun-shades for side windows (PR-3Y8)
+00256 - SAFE-motor in door lock
+00512 - Mirror fold in function (PR-6XE/6XF/6XK/6XL)
+01024 - Outside mirror automatic dimming (PR-6XJ/6XK/6XL/6XM)
+02048 - Pinch protection always active
+04096 - Closing aid (PR-GZ2)
+08192 - Seat memory for drivrs seat (PR-3PN)
+16384 - Seat memory for passenger seat (PR-3PN)
+32768 - Child safety lock deactivated at rear door open
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{Instrument Cluster}

Control module coding
Select 17 (Instrument Cluster)
Coding -> Function 07
??xxx: Extra-Options
+01 - Quattro (2nd fuel tank map)
+04 - Vehicle with clutch (no auto. transmission)
+08 - 2nd tire size (difference between summer and winter tires)
+16 - Tire Monitoring System (MY 2005 >)
xx?xx: Country-Setting
0 - Germany (D)
1 - Rest of World (RoW - left hand)
2 - USA (US)
3 - Canada (CAN)
4 - Grea britain (GB)
5 - Japan (JP - left hand)
6 - Arabian states
7 - Australia (AUS)
8 - Rest of World (RoW - right hand)
9 - Japan (JP - right hand)
xxx?x: Seat belt warning
Note: Options 3-6 are only avialiable for MY 2005 and above.
	0
	no seat belt warning

	1
	seat belt warning Europe-NCAP
Optical durable warning, acustical warning for 91 seconds activ.

	2
	seat belt warning USA and Canada old 
Optical and acustical warning for 6 seconds

	3
	seat belt warning USA and Canada NAR neu
Optical durable warning, acustical warning all 30 seconds

	4
	seat belt warning Europe-NCAP (incl. passenger)
Optical durable warning, acustical warning for 91 seconds activ.

	5
	seat belt warning USA and Canada old (incl. passenger)
Optical and acustical warning for 6 seconds

	6
	seat belt warning USA and Canada NAR new (incl. passenger)
Optical durable warning, acustical warning all 30 seconds


xxxx?: Illumination options
Note: Options 4-9 are only avialiable for MY 2005 and above. Options 0-4 with parking light LED off, options 5-9 with parking ligh LED on.
0 - Needles and Scales OFF (term.15 on / term.58 off)
1 - Needles ON, Scales OFF (term.15 on / term.58 off)
2 - Needles OFF, Scales ON (term.15 on / term.58 off)
3 - Needles and Scales ON (term.15 on / term.58 off)
4 - Needles and Scales ON (term. 15 / term.58 off)
5 - Needles and Scales OFF(term.15 on / term.58 off)
6 - Needles ON, Scales OFF(term.15 on / term.58 off)
7 - Needles OFF, Scales ON (term.15 on / term.58 off)
8 - Needles and Scales ON (term.15 on / term.58 off)
9 - Needles and Scales ON (term.15 / term.58 off)
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{Level Control System}

Control module basic setting
See the Ross-Tech's How-To:
Suspension Level Control Calibration
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{Trailer}

Control module coding
Select 69 (Trailer)
Coding -> Function 07
000?x: Hitch System
0 - Trailer Connection Unit (removable)
1 - Trailer Connection Unit (swivelling - automatic running)
2 - Trailer Connection Unit (swivelling - manual running)
000x?: Country
1 - Rest of World (RoW)
2 - USA
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{Transmission Electronics}

Control module coding
Select 02 (Transmission Electronics)
Coding -> Function 07
 

{Audi TT (8N)}
 The following control modules are build into the TT (8N) (items shown in orange have been described in the text that follows.  Click on an orange item to go directly to that section):
- Airbag
- Autom. Transmission
- Auxiliary Heater
- Brake Electronics
- Central Locking/Comfort System
- Engine Electronics
- Headlight Aim Control
- Heating/Air Conditioning
- Instrument Cluster
- Interior Monitoring
- Radio (Generation I)
- Radio-/Navigation (RNS-E)
- Telephone 
{Instrument Cluster}

Control Module Coding
Select 17 (Instrument Cluster)
Coding -> Function 07
??xxx: Equipment (through MY 1999)
+00 - No extra equipment
+01 - Bigger fuel tank (quattro)
+02 - Seatbelt warning active
+04 - Washer fluid warning active
+16 - Secondary display active (radio/navigation w/o CAN)
??xxx: Equipment (from MY 2000)
+00 - No extra equipment
+01 - Bigger fuel tank (quattro)
+02 - Seatbelt warning active
+04 - Manual Transmission (02M)
+16 - Secondary display active (radio/navigation w/o CAN)
xx?xx: Country
0 - Germany (D)
1 - Rest of World (left hand steering - RoW)
2 - USA (US)
3 - Canada (CDN)
4 - Great Britain (GB)
5 - Japan (left hand steering - JP)
6 - Saudi Arabia (SA)
7 - Australia (AUS)
8 - Rest of World (right hand steering - RoW)
9 - Japan (right hand steering - JP)
xxx?x: Cylinder
4 - 4-Cylinder
6 - 6-Cylinder
xxxx?: Engine
2 - Gasoline Engine
4 - Turbo Engine
Control Module Adaptation
Select 17 (Instrument Cluster)
Adaptation -> Function 10
-> Channel 04 (Language)
00001 - German
00002 - English
00003 - French
00004 - Italian
00005 - Spanish
00006 - Portuguese
