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I ith keyless entry system

101999

With keyless entry system

Insert remote control in ignition slot
DO NOT depress any pedals

Press and hold start/stop button for approximately 10 seconds to switch ignition ON.

Repeatedly press button [A] 101999 until the 'spanner’ symbol flashes and the distance remaining to the next senice appears in the
‘odometer display.

Press and hold button [B] for approximately 10 seconds unti the new senvce intenval is displayed

Release button [B]

Press start/stop button to switch ignition OFF
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