	Servicing fuel injection system

Injection pump with two-part sprocket


	 

	
	

	Injection pump with one-part sprocket

=>Page 23-2
· Idling speed boost actuator 

· ◆ Pneumatic for vehicles with air conditioner 

· ◆ Adjusting => Page 23-40 

2. Bracket 

3. 10 Nm 

4. 20 Nm 

5. Clamping piece 

6. Injection pump sprocket 

· ◆ Two part 
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	1. 25 Nm 

2. Clamping piece 

3. Protective cap 

4. Bracket 

5. Idling speed boost actuator (N123) 

· ◆ Electric for vehicles without air conditioner 

· ◆ Adjusting => Page 23-40 

6. Commencement of injection valve (N108) 

· ◆ Checking =>Page 01-16, final control diagnosis 

7. Injection period sender (G175) 

· ◆ Tighten to 25 Nm 

8. Sealing ring 

· ◆ Renew 
	


